Debug:(toolbox.cpp:15, ) ToolBox Start.....
Debug:(qunp.cpp:1707, ) false "COM9" "COM9"
Debug:(qnfc.cpp:604, ) 93
Debug:(qnfc.cpp:809, ) deal_with_nfc_ack satus:  0
Debug:(qnfc.cpp:840, ) start recv flash

Debug:(qnfc.cpp:848, ) ===recv_len = 1158, recv_num = 19

Debug:(qnfc.cpp:604, ) 99
Debug:(qnfc.cpp:604, ) 99
Debug:(qnfc.cpp:604, ) 99
Debug:(qnfc.cpp:604, ) 99
Debug:(qnfc.cpp:604, ) 99
Debug:(qnfc.cpp:604, ) 99
Debug:(qnfc.cpp:604, ) 99
Debug:(qnfc.cpp:604, ) 99
Debug:(qnfc.cpp:604, ) 99
Debug:(qnfc.cpp:604, ) 99
Debug:(qnfc.cpp:604, ) 99
Debug:(qnfc.cpp:604, ) 99
Debug:(qnfc.cpp:604, ) 99
Debug:(qnfc.cpp:604, ) 99
Debug:(qnfc.cpp:604, ) 99
Debug:(qnfc.cpp:604, ) 99
Debug:(qnfc.cpp:604, ) 99
Debug:(qnfc.cpp:604, ) 99
Debug:(qnfc.cpp:604, ) 99
Debug:(qunp.cpp:1818, ) 
Debug:(qunp.cpp:1826, ) "WS202"
Debug:(qnfc.cpp:155, ) "WS202" 0
Debug:(qnfc.cpp:159, ) ## imagesize: 1158

Debug:(qnfc.cpp:160, ) ############# 8758975b

Debug:(qnfc.cpp:161, ) ############# 8758975b

Debug:(connectting.cpp:69, ) Device Connect Success
Debug:(qunp.cpp:1818, ) 
Debug:(qunp.cpp:1826, ) "WS202"
Debug:(qunp.cpp:1856, ) pn--- 470M

Debug:(qunp.cpp:614, ) ===device oem:

Debug:(connectting.cpp:90, ) product name pn:  "WS202-470M"
Debug:(connectting.cpp:102, ) close serial port
Debug:(toolbox.cpp:322, ) product name: "WS202-470M" "01.01" "1.0" 0
Debug:(toolbox.cpp:342, ) "model_page"
Debug:(toolbox.cpp:860, ) 
Debug:(ws202dealthread.cpp:19, ) Thread id: 0x3458
Debug:(ws202dealthread.cpp:122, ) request type:0
Debug:(qunpbasic.cpp:1831, ) false "COM9" "COM9"
Debug:(qunpws202.cpp:962, ) pn--- 470M

Debug:(qunpws202.cpp:176, ) ===device oem:

Debug:(qunpws202.cpp:1072, ) pn3--- 

Debug:(qunpws202.cpp:314, ) read lorawan param:80 pos 11 len 8

Debug:(qunpws202.cpp:236, ) PARAM_USER_CONFIG 1 0 80

Debug:(qunpbasic.cpp:1918, ) false
Debug:(:0, ) QObject::connect: No such signal LogWnd::close()
Debug:(:0, ) QObject::connect:  (sender name:   'LogWnd')
Debug:(:0, ) QObject::connect:  (receiver name: 'LogWnd')
Debug:(ws202dealthread.cpp:122, ) request type:2
Debug:(qunpbasic.cpp:1831, ) false "COM9" "COM9"
Debug:(qunpws202.cpp:438, ) [debug]: read PARAM_LED_MODE = 0

Debug:(qunpws202.cpp:452, ) [debug]: read PARAM_PIR_IDLE = 102

Debug:(qunpws202.cpp:445, ) [debug]: read PARAM_BATTERY_CYCLE = 18060

Debug:(qunpws202.cpp:236, ) PARAM_USER_CONFIG 1 0 80

Debug:(ws202dealthread.cpp:402, ) [PARAM_USER_CONFIG ] cfg.sensor1.enable: 1

Debug:(qunpws202.cpp:266, ) id:1 
Debug:(qunpws202.cpp:277, ) [debug]: read PARAM_HT_ALARM datasize:17
Debug:(ws202dealthread.cpp:407, ) [alarm params ] over: 102 , below: 21

Debug:(qunpws202.cpp:314, ) read lorawan param:80 pos 205 len 41

Debug:(qunpws202.cpp:459, ) ###########################  12 0 "00"
Debug:(qunpws202.cpp:460, ) ###########################  12 0 "00"
Debug:(qunpbasic.cpp:1918, ) false
