Thanks for purchasing PLANET IGT-900-1T1S Media Converter.
This document provides the firmware release note and the history of the product.

Date of Release

Firmware version: 1.440b221017
Released on 10/17/22

This firmware includes the following modification:

A. Bug Fixed -
Authentication request appears twice when logging into the console of the IGS-900-1T1S via SSH (Secure Shell) with the previous firmware version (v1.440b211210). This issue has been fixed with the firmware update in version 1.440b221017.

B. Function Added -
N/A


[Upgrade Requirements]:

1. The latest firmware version (v1.440b221017) of IGT-900-1T1S 
2. The IGT-900-1T1S Media Converter
3. Workstation with web browser


[Upgrade procedure]:

1. Connect an RJ45 UTP cable to the Media Converter.

2. Login is required to access the Web interface after the device has been booted successfully. The factory default username and password are both "admin". 

3. When web management screen appears, click the Maintenance button on the banner above. 

4. Click Switch Maintenance on the sidebar to the left and then click Web Firmware Upgrade.
In the middle of the main screen, you will see “Choose File” and “Upload File” buttons. 

5. Click “Choose File” to browse the downloaded firmware file and then click “Upload File” to perform firmware update. “Firmware Upgrade in Progress” appears in the main screen.

6. Do not power off the device until the upgrade process is completed.

7. Once the firmware is loaded into the system successfully, the device will reboot and load the new firmware during the startup.

8. When the device reboot completes, get back to the web browser. In the main screen, click "System”,“Management”,and then“System Information”. In the bottom of System Information table, check the“Software Version”to confirm if the firmware has been upgraded successfully.


Sincerely,
PLANET Technical Support Team
Http://www.planet.com.tw
